turnon
Prev | Orchestra Opcodes and Operators | Next

## turnon

turnon — Activate an instrument for an indefinite time.

## Description

Activate an instrument for an indefinite time.

## Syntax

    turnon insnum [, itime]

## Initialization

insnum -- instrument number to be activated

itime (optional, default=0) -- delay, in seconds, after which instrument insnum will be activated. Default is 0.

## Performance

turnon activates instrument insnum after a delay of itime seconds, or immediately if itime is not specified. Instrument is active until explicitly turned off. (See turnoff.)

## Examples

Here is an example of the turnon opcode. It uses the files turnon.csd.

Example 1133. Example of the turnon opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac ;;;realtime audio out
    ;-iadc ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o turnon.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; by Stefano Cucchi 2020 and Richard Boulanger

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs = 1

    gasend1 init 0
    gasend2 init 0

    turnon 100
    turnon 101

    instr 1

    abar barmodel 2, 2, p4, 0.000001, 0.0103, 20, p5, p6, p7
    kenvelope expseg 1, p3, .01
    abar = abar * kenvelope * p8
    ; NO local output

    gasend1 = gasend1 + abar*p8
    gasend2 = gasend2 + abar*p8

    endin

    instr 2

    idenStart = p4
    kdensity expseg p4, p3, 0.001
    apulse mpulse 1, kdensity
    kenvelope expseg 1, p3, .001
    apulse = apulse * kenvelope * p5
    ; NO local output

    gasend1 = gasend1 + apulse
    gasend2 = gasend2 + apulse

    endin

    instr dry

    idryLeft = p4
    idryRight = p5
    kgate adsr .01,.01,1,0
    outs (gasend1*kgate) * p4, (gasend2*kgate) * p5

    endin

    instr 100

    aphaser phaser1 gasend1, 4700, 1000, -0.8
    arevphaser reverb aphaser, 1.618
    outs arevphaser * 0.2, arevphaser * 0.2
    clear gasend1

    endin

    instr 101

    afold fold gasend2, 26
    adelfoldL multitap afold, 0.62, 0.52, 1.19, 0.44
    adelfoldR multitap afold, 0.94, 0.64, 1.42, 0.54
    outs adelfoldL * 0.5, adelfoldR * 0.5
    clear gasend2

    endin

    </CsInstruments>
    <CsScore>

    i2 0 6 .07  1

    i "dry" 0 2 .87 .2

    i1 3 4 10 0.13 300 0.3 0.8

    i2 7 5 .007  1

    i "dry" 7 3 .12 .86

    i1 11 9 09 0.09 400 0.23 0.78

    i2 15 9 .01 1

    i "dry" 15 12 .94 .09

    s

    i "dry" 0 26.9 .68 .48 ; lowered

    i 2 0.0 4 .07  1
    i 2 0.1 4 .02  1

    i 1 0.21 1 08 0.13 300 0.3 0.8
    i 1 2 2 14 0.02 500 0.2 0.7

    i 2 2 5 .06  0.8 ; lowered
    i 2 4 5 .05  0.7 ; lowered
    i 2 4 6 .01  0.6 ; lowered

    i 1 4.3 3 9 0.08 1145 0.1 0.5 ; lowered
    i 1 4.5 3 11 0.10 245 0.2 0.4 ; lowered

    i 1 8.00 7 08 0.11 125 0.1 0.6
    i 1 8.01 6 28 0.13 280 0.3 0.8
    i 1 8.02 5 39 0.02 600 0.2 0.7
    i 1 8.03 4 39 0.02 600 0.2 0.7

    i 2 8.24 18 .09 1
    i 2 8.75 11 .05 1
    i 2 8.99 4 .01 1

    i 1 18 9 8.1 0.12 105 0.12 0.56
    i 1 18.01 8 8.8 0.13 205 0.52 0.46

    i 1 18.02 7 8.2 0.15 745 0.42 0.26
    i 1 18.03 11 8.3 0.14 905 0.62 0.36

    i "dry" 25 .85 .32 .38

    i 2 25 5 .71 1

    i "dry" 27 .74 .62 .68

    i 2 27 6 .11 1

    i "dry" 32.3 .42 .32 .38

    i 2 32.3 14 .005  1

    i 1 36 13 9.9 0.233 333 0.23 0.63
    i 1 39 12 8.9 0.323 403 0.34 0.53
    i 1 42 10 7.8 0.123 283 0.42 0.73

    i 1 48.01 9 8.11 0.122 108 0.13 0.54
    i 1 48.03 8 8.82 0.135 208 0.50 0.44
    i 1 48.05 7 8.23 0.158 748 0.40 0.24
    i 1 48.08 11 8.35 0.147 908 0.60 0.34

    e 60 ; score extended to allow for reverb and multitap tails to ring out

    ; keeping instr 100 and instr 101 "turned on" for 60 seconds

    </CsScore>
    </CsoundSynthesizer>

## See Also

turnoff, turnoff2

Prev | Up | Next
turnoff3 | Home | tvconv