fmanal
Prev | Orchestra Opcodes and Operators | Next

## fmanal

fmanal — AM/FM analysis from quadrature signal.

## Description

This opcode attempts to extract the AM and FM signals off a quadrature signal (e.g. from a Hilbert transform).

## Syntax

    am, af fmanal are, aim

## Performance

are -- real (cosine-phase) input signal

aim -- imaginary (sine-phase) input signal

am -- amplitude modulation envelope

af -- frequency modulation envelope

fmanal takes a signal in quadrature (real, imag) and outputs the estimate AM and FM signals. The former is the modulus of each input sample pair (|re + j*im|) and the latter the derivative of arg(re + j*im). Each sample of the output is the estimated instantaneous amplitude and frequency of the input signal.

## Example

Here is an example of the fmanal opcode. It uses the file fmanal.csd.

Example 349. Example of the fmanal opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 64
    nchnls = 2
    0dbfs = 1

    instr 1

    asig oscili p4, p5
    a1,a2 hilbert2 asig,1024,256
    am,afm fmanal a1,a2
    ktrig metro 2
    printf "AM=%.3f FM=%.1f\n",ktrig,k(am),k(afm)
      outs a1, a2

    endin

    </CsInstruments>
    <CsScore>
    i1 0 10 0.5 440
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Victor Lazzarini
2017

Prev | Up | Next
FLxyin | Home | fmax