STKBlowHole
Prev | Orchestra Opcodes and Operators | Next

## STKBlowHole

STKBlowHole — STK clarinet physical model with one register hole and one tonehole.

## Description

Plugin opcode in stkopd. This opcode is part of the plugin repository and has to be installed separately. The plugin repository can be found here: https://github.com/csound/plugins

This opcode is based on the clarinet model, with the addition of a two-port register hole and a three-port dynamic tonehole implementation.

In this implementation, the distances between the reed/register hole and tonehole/bell are fixed. As a result, both the tonehole and register hole will have variable influence on the playing frequency, which is dependent on the length of the air column. In addition, the highest playing freqeuency is limited by these fixed lengths.

## Syntax

    asignal STKBlowHole ifrequency, iamplitude, [kreed, kv1[, knoise, kv2[, khole, kv3[, kreg, kv4[, kbreath, kv5]]]]]

## Initialization

ifrequency -- Frequency of note played, in Hertz.

iamplitude -- Amplitude of note played (range 0-1).

## Performance

kreed -- controller 2, stiffness of reed. Value range of kv1 is 0-127.

knoise -- controller 4, gain of noise. Value range of kv2 is 0-127.

khole -- controller 11, state of tonehole. Value range of kv3 is 0-127.

kreg -- controller 1, state of register. Value range of kv4 is 0-127.

kbreath -- controller 128, breath pressure. Value range of kv5 is 0-127.

| Notes
The code for this opcode is taken directly from the BlowHole class in the Synthesis Toolkit in C++ by Perry R. Cook and Gary P. Scavone. More on the STK classes can be found here: https://ccrma.stanford.edu/software/stk/classes.html kc1, kv1, kc2, kv2, kc3, kv3, kc4, kv4, kc5, kv5, kc6, kv6, kc7, kv7, kc8, kv8 -- Up to 8 optional k-rate controller pairs for the STK opcodes. Each controller pair consists of a controller number (kc) followed by a controller value (kv). Both the controller numbers and the controller values are krate variables. However, during a performance, normally the controller numbers stay fixed while the corresponding controller values may change at any time. The order of the controller pair is arbitrary, as long as they are after iamplitude. Also, it is not needed that all controller pairs are used.

## Examples

Here is an example of the STKBlowHole opcode. It uses the file STKBlowHole.csd.

Example 1014. Example of the STKBlowHole opcode.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if RT audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o STKBlowHole.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    ipch	=	p4
    kv1	=	p7						;stiffness of reed
    kv3	line	p5, p3, p6					;state of tonehole

    asig	STKBlowHole	cpspch(ipch), 1, 2, kv1, 4, 100, 11, kv3, 1, 10, 128, 100
    	outs	asig, asig
    endin

    </CsInstruments>
    <CsScore>

    i 1 0 4 10.00 20 127 100
    i 1 + 7 6.09 120  0  10
    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Michael Gogins (after Perry Cook)
Irreducible Productions
New York, NY

New in Csound version 5.11

Prev | Up | Next
STKBlowBotl | Home | STKBowed