endop
Prev | Orchestra Opcodes and Operators | Next

## endop

endop — Marks the end of an user-defined opcode block.

## Description

Marks the end of an user-defined opcode block.

## Syntax

                endop

## Performance

The syntax of a user-defined opcode block is as follows:

    opcode  name, outtypes, intypes
    xinarg1 [, xinarg2] [, xinarg3] ... [xinargN]  xin
    [setksmps  iksmps]
    ... the rest of the instrument's code.
    xout  xoutarg1 [, xoutarg2] [, xoutarg3] ... [xoutargN]
    endop

The new opcode can then be used with the usual syntax:

    [xinarg1] [, xinarg2] ... [xinargN]  name  [xoutarg1] [, xoutarg2] ... [xoutargN] [, iksmps]

## Examples

Here is an example of the endop opcode. It uses the file endop.csd.

Example 265. Example of the endop opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac     ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o endop.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs = 1

    /* example opcode 1: simple oscillator */

            opcode Oscillator, a, kk

    kamp, kcps      xin             ; read input parameters
    a1      vco2 kamp, kcps         ; sawtooth oscillator
            xout a1                 ; write output

            endop

    /* example opcode 2: lowpass filter with local ksmps */

            opcode Lowpass, a, akk

            setksmps 1              ; need sr=kr
    ain, ka1, ka2   xin             ; read input parameters
    aout    init 0                  ; initialize output
    aout    =  ain*ka1 + aout*ka2   ; simple tone-like filter
            xout aout               ; write output

            endop

    /* example opcode 3: recursive call */

            opcode RecursiveLowpass, a, akkpp

    ain, ka1, ka2, idep, icnt       xin     ; read input parameters
            if (icnt >= idep) goto skip1    ; check if max depth reached
    ain     RecursiveLowpass ain, ka1, ka2, idep, icnt + 1
    skip1:
    aout    Lowpass ain, ka1, ka2           ; call filter
            xout aout                       ; write output

            endop

    /* example opcode 4: de-click envelope */

            opcode DeClick, a, a

    ain     xin
    aenv    linseg 0, 0.02, 1, p3 - 0.05, 1, 0.02, 0, 0.01, 0
            xout ain * aenv         ; apply envelope and write output

            endop

    /* instr 1 uses the example opcodes */

            instr 1

    kamp    =  .6                ; amplitude
    kcps    expon 50, p3, 500       ; pitch
    a1      Oscillator kamp, kcps                   ; call oscillator
    kflt    linseg 0.4, 1.5, 0.4, 1, 0.8, 1.5, 0.8  ; filter envelope
    a1      RecursiveLowpass a1, kflt, 1 - kflt, 10 ; 10th order lowpass
    a1      DeClick a1
            outs a1, a1

    endin
    </CsInstruments>
    <CsScore>

    i 1 0 4
    e

    </CsScore>
    </CsoundSynthesizer>

## See Also

opcode, setksmps, xin, xout

More information on this opcode: http://www.csoundjournal.com/2006summer/controlFlow_part2.html , written by Steven Yi

The user-defined opcode page: http://www.csounds.com/udo/ , maintained by Steven Yi

## Credits

Author: Istvan Varga, 2002; based on code by Matt J. Ingalls

New in version 4.22

Prev | Up | Next
endin | Home | envlpx