expseg
Prev | Orchestra Opcodes and Operators | Next

## expseg

expseg — Trace a series of exponential segments between specified points.

## Description

Trace a series of exponential segments between specified points.

## Syntax

    ares expseg ia, idur1, ib [, idur2] [, ic] [...]

    kres expseg ia, idur1, ib [, idur2] [, ic] [...]

## Initialization

ia -- starting value. Zero is illegal for exponentials.

ib, ic, etc. -- value after dur1 seconds, etc. For exponentials, must be non-zero and must agree in sign with ia.

idur1 -- duration in seconds of first segment. A zero or negative value will cause all initialization to be skipped.

idur2, idur3, etc. -- duration in seconds of subsequent segments. A zero or negative value will terminate the initialization process with the preceding point, permitting the last-defined line or curve to be continued indefinitely in performance. The default is zero.

## Performance

These units generate control or audio signals whose values can pass through 2 or more specified points. The sum of dur values may or may not equal the instrument's performance time: a shorter performance will truncate the specified pattern, while a longer one will cause the last-defined segment to continue on in the same direction.

Note that the expseg opcode does not operate correctly at audio rate when segments are shorter than a k-period. Try the expsega opcode instead.

## Examples

Here is an example of the expseg opcode. It uses the file expseg.csd.

Example 282. Example of the expseg opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    ; Audio out   Audio in
    -odac             ;;;RT audio out
    ; For Non-realtime ouput leave only the line below:
    ;-o expseg.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    ; by Kevin Conder, additions by Menno Knevel 2021

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    kcps = cpspch(p4)                           ; p4 = frequency in pitch-class notation.
    kenv expseg 0.01, p3*0.25, 1, p3*0.75, 0.001 ; amplitude envelope.
    kamp = kenv
    a1 oscili kamp, kcps
    outs a1, a1

    endin

    </CsInstruments>
    <CsScore>

    i 1 0 0.5 8.00
    i 1 1 0.5 8.01
    i 1 2 0.5 8.02
    i 1 3 2.0 8.03
    e
    </CsScore>
    </CsoundSynthesizer>

## See Also

expon, expsega, expsegr, line, linseg, triglinseg, trigexpseg, linsegr, transeg

## Credits

Author: Gabriel Maldonado

New in Csound 3.57

Prev | Up | Next
exprandi | Home | expsega