mvclpf4
Prev | Orchestra Opcodes and Operators | Next

## mvclpf4

mvclpf4 — Moog voltage-controlled lowpass filter emulation.

## Description

Mvclpf4 is an digital implementation of the 4th-order (24 dB/oct) Moog ladder filter originally written by Fons Andriaensen. It is a version of the mvclpf3 opcode with four outputs, for 6dB, 12dB, 18dB, and 24 dB/octave responses.

## Syntax

    asig1,asig2,asig3,asig4 mvclpf4 ain, xcf, xres[, istor]

## Initialization

istor --initial disposition of internal data space. Since filtering incorporates a feedback loop of previous output, the initial status of the storage space used is significant. A zero value will clear the space; a non-zero value will allow previous information to remain. The default value is 0.

## Performance

asig1 -- 6dB/oct low-pass response output.

asig2 -- 12dB/oct low-pass response output.

asig3 -- 18dB/oct low-pass response output..

asig4 -- 24dB/oct low-pass response output.

ain -- input signal.

xcf -- filter cutoff frequency. The useful range is around six octaves below and above middle C (pch 8.00).

xres -- resonance, limited to the interval [0,1].

## Examples

Here is an example of the mvclpf4 opcode. It uses the file mvclpf4.csd.

Example 646. Example of the mvclpf4 opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    -odac
    </CsOptions>
    <CsInstruments>
    0dbfs = 1

    instr 1
     asig[] init 4
     kenv linen p4,0.1,p3,0.1
     ain rand kenv
     kfr expon 220, p3, 1760
     asig[0],asig[1],asig[2],asig[3] mvclpf4 ain,kfr,0.9
      out asig[p5]
    endin

    </CsInstruments>
    <CsScore>
    i1 0 5 0.9 0
    i1 + 5 0.9 1
    i1 + 5 0.9 2
    i1 + 5 0.9 3
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: Fons Andriaensen,
ported to Csound by Victor Lazzarini
January 2016

New in version 6.07

January 2016.

Prev | Up | Next
mvclpf3 | Home | mvmfilter