lfo
Prev | Orchestra Opcodes and Operators | Next

## lfo

lfo — A low frequency oscillator of various shapes.

## Description

A low frequency oscillator of various shapes.

## Syntax

    kres lfo kamp, kcps [, itype]

    ares lfo kamp, kcps [, itype]

## Initialization

itype (optional, default=0) -- determine the waveform of the oscillator. Default is 0.

- itype = 0 - sine

- itype = 1 - triangles

- itype = 2 - square (bipolar)

- itype = 3 - square (unipolar)

- itype = 4 - saw-tooth

- itype = 5 - saw-tooth(down)

The sine wave is implemented as a 4096 table and linear interpolation. The others are calculated.

## Performance

kamp -- amplitude of output

kcps -- frequency of oscillator

## Examples

Here is an example of the lfo opcode. It uses the file lfo.csd.

Example 497. Example of the lfo opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>
    ; Select audio/midi flags here according to platform
    -odac      ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o lfo.wav -W ;;; for file output any platform
    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1

    instr 1

    kcps  = 5
    itype = p4	;lfo type

    klfo line 0, p3, 20
    al   lfo klfo, kcps, itype
    asig poscil .5, 220+al, 1
         outs asig, asig

    endin
    </CsInstruments>
    <CsScore>
    ; sine wave.
    f 1 0 32768 10 1

    i 1 0 3 0	;lfo = sine
    i 1 + 3 2	;lfo = square
    i 1 + 3 5	;lfo = saw-tooth down
    e
    </CsScore>
    </CsoundSynthesizer>

Here is another example of the lfo opcode. It uses the file lfo-advanced.csd.

Example 498. Advanced example of the lfo opcode.

See the sections Real-time Audio and Command Line Flags for more information on using command line flags.

    <CsoundSynthesizer>
    <CsOptions>

    ; Select audio/midi flags here according to platform
    -odac      ;;;realtime audio out
    ;-iadc    ;;;uncomment -iadc if realtime audio input is needed too
    ; For Non-realtime ouput leave only the line below:
    ; -o lfo_advanced.wav -W ;;; for file output any platform

    ; By Stefano Cucchi 2020

    </CsOptions>
    <CsInstruments>

    sr = 44100
    ksmps = 32
    nchnls = 2
    0dbfs  = 1
    instr 1

    ; LFO 1
    kAmpLFO1 linseg p6, p3, p7
    kFreqLFO1 linseg p8, p3, p9
    kLFO1 lfo kAmpLFO1, kFreqLFO1, p10

    ; LFO 2
    kAmpLFO2 linseg p7, p3, p6
    kFreqLFO2 linseg p9, p3, p8
    kLFO2 lfo kAmpLFO2, kFreqLFO1, p11

    ; AUDIO SIGNAL
    asig1 oscili p4+kLFO1, p5+kLFO2,1

    ; LFO DELAY
    kAmpDELAY1 lfo, 100, 1.35, 1
    kAmpDELAY1 = kAmpDELAY1 + 50

    ; DELAY SIGNAL
    adel1 vdelay asig1, kAmpDELAY1, 500

    kdeclick linseg 0, 1.5, p12, p3-3, p12, 1.5, 0
    outch 1, (asig1  + (adel1 *0.3)) * kdeclick
    outch 2, (asig1  + (adel1 *0.3)) * kdeclick

    endin

    </CsInstruments>
    <CsScore>

    f 1 0 4096 10 1 0.3 0.2 0.1 0.03 0 0.3

    i1 0 8 0.3 250 0.22 0.65 3 6 0 3 0.8
    i1 8 8 0.3 123 0.12 10.85 70 6 1 5 0.09

    e
    </CsScore>
    </CsoundSynthesizer>

## Credits

Author: John ffitch
University of Bath/Codemist Ltd.
Bath, UK
November 1998

New in Csound version 3.491

Prev | Up | Next
lenarray | Home | lfsr