Steps taken to evaluate wolfSSL with the following:

Required Software for this guide:
IAR Embedded Workbench IDE - ARM v7.60.1 (or similar version)
embOS (version that supports your CPU)
wolfssl (latest version)

#----------------------------------------------------------------------------#
# SECTION 1:
# Setting up the file system
#----------------------------------------------------------------------------#

1. Browse to wolfssl/IDE/IAR-EWARM/embOS/
    a. copy/paste the directory custom_port and re-name it to the CPU
       you intend to target. For now we will just use the term CUSTOM_DIR
       to signify a copy of the custom_port directory

#----------------------------------------------------------------------------#
# SECTION 2:
# Create wolfcrypt_lib.a
#----------------------------------------------------------------------------#

1. Open IAR Workbench -> Project -> Create New Project -> Empty Project
    c. Browse to CUSTOM_DIR/wolfcrypt_lib_custom_port/ (from section 1)
    d. Called it "wolfcrypt_lib" and hit "Save"

2. Go to Project -> Add Group...
    a. call group wolfcrypt_sources

3. Right click on wolfcrypt_sources group -> Add -> Add Files...

4. Browse to wolfssl/wolfcrypt/src directory and select the following files:

 #---------------------------------------------#
 #     aes.c                   memory.c        #
 #     asn.c                   misc.c          #
 #     chacha.c                poly1305.c      #
 #     chacha20_poly1305.c     pwdbased.c      #
 #     coding.c                rabbit.c        #
 #     des3.c                  random.c        #
 #     dh.c                    rsa.c           #
 #     dsa.c                   sha.c           #
 #     ecc.c                   sha256.c        #
 #     hash.c                  sha512.c        #
 #     hmac.c                  tfm.c           #
 #     md4.c                   wc_encrypt.c    #
 #     md5.c                   wc_port.c       #
 #---------------------------------------------#

5. Once those are all added go to
                    Project -> Properties C/C++ Compiler -> Preprocessor (Tab)
    a. In the field "Defined symbols:" add WOLFSSL_USER_SETTINGS
    b. In the field "Additional include directories:"
        put in this line: $PROJ_DIR$\..\..\..\..\..\
		   and this line: $PROJ_DIR$\..\custom_port_user_settings
		#---------------------------------------------
        #(Or alternately you can use the browse option to navigate to
        #C:\<path-to>\wolfssl and
        #C:\<path-to>\wolfssl\IDE\IAR-EWARM\CUSTOM_DIR\
        #                                        custom_port_user_settings\)
		#(If you ever need to change or customize your build settings this
	    #is the file that should be modified:
	    #CUSTOM_DIR\custom_port_user_settings\user_settings.h)
        #---------------------------------------------

7. In Project -> Options -> General Options -> Output (Tab)
    Check the option for "Library" instead of "Executable"
    Click "OK"

8. Go to Project -> Rebuild all (The library should build)

9. Confirm the library is now located here:
    C:\<path to>\wolfssl\IDE\IAR-EWARM\CUSTOM_DIR\wolfcrypt_lib_custom_port\
                                                    Debug\Exe\wolfcrypt_lib.a

We are now set to link to this library in the evaluation project

#----------------------------------------------------------------------------#
# SECTION 3:
# Evaluate wolfcrypt tests in embOS project:
#----------------------------------------------------------------------------#


1. go to embOS website and download a trial for your platform
   https://www.segger.com/downloads/embos ->
                                     embOS trial for Cortex-M and IAR compiler

2. After downloading, extract the zip to:
                  C:\<path-to>\wolfssl\IDE\IAR-EWARM\embOS\extract_trial_here\

3. Open IAR Workbench -> Project -> Create New Project -> Empty Project
    c. Browse to CUSTOM_DIR\wolfcrypt_test_custom_port\ (from section 1)
    d. Called it "wolfcrypt_test" and hit "Save"

4. Go to Project -> Options -> C/C++ Compiler -> Preprocessor (Tab)
    a. Add these to the field "Defined symbols:"
        DEBUG=1
        __CPU-YOU-ARE-TARGETING__ (For example: __SAMV71Q21__)
        WOLFSSL_USER_SETTINGS

    b. Now in the field "Additional include directories:"
        $PROJ_DIR$\..\..\..\..\..\
		$PROJ_DIR$\..\custom_port_user_settings
		#---------------------------------------------
        #(Or alternately you can use the browse option to navigate to
        #C:\<path-to>\wolfssl and
        #C:\<path-to>\wolfssl\IDE\IAR-EWARM\CUSTOM_DIR\
        #                                        custom_port_user_settings\)
        #---------------------------------------------

5. Go to Project -> Options -> Linker -> Library (Tab)
    Add to the field "Additional libraries:"
    $PROJ_DIR$\..\embOS_wolfcrypt_lib_SAMV71_XULT\Debug\Exe\wolfcrypt_lib.a
    $PROJ_DIR$\..\..\extract_trial_here\Start\Lib\os7m_tlv_dp.a

6. The main project file is located here:
      CUSTOM_DIR\wolfcrypt_test_custom_port\Application\runWolfcryptTests.c

7. Right Click the project name: Add -> Add Group
                                           add a group called "Application"
8. Right Click that group and Add -> Add files
                            browse to the main project file in step 5 above

9. Create Groups and add files for your CPU's support. These will be .c
   files found in the extracted directory in two places:

   extract_trial_here\Start\BoardSupport\<vendor>\<CPU>\DeviceSupport
   extract_trial_here\Start\BoardSupport\<vendor>\<CPU>\Setup
   #---------------------------------------------
   # For example:
   # extract_trial_here\Start\BoardSupport\Atmel\SAMV71_XPlainedUltra\
   #                                                          DeviceSupport
   # extract_trial_here\Start\BoardSupport\Atmel\SAMV71_XPlainedUltra\Setup
   #---------------------------------------------
   
10. To get Logging working for seeing test results:
    a. Go to Project -> Options -> General Options -> Library Configuration
    b. In the field "Library low-level interface implementation"
        Check the radio button for Semihosted
        Then in the inner field marked "stdout/stderr"
            Check the radio button for "Via semihosting" and click "OK"

11. Now we're ready to build and debug the project.
    a. Project -> Options -> Debugger
        In the field marked "Driver" Select drop-down and choose J-Link/J-Trace
        Click "OK"
    b. Project -> Rebuild All
    c. Connect your Cortex-M evaluation board to j-Trace and j-Trace to PC
    d. Connect the micro-USB to the debug port of the Cortex-M and PC for power
    e. Project -> Download and Debug

12. Once the Debug environment spawns go to View -> Terminal I/O
    This is where the "printf" to stdout will be directed

13. In the Debug Menu bar look for the little square with three arrows pointing
    to the right. When you mouse over it should say "GO"
    Click this option and in the Terminal I/O Window you should see something
    like this (depends on which functionality you set in user_settings.h)

    SEE NOTE 1 BELOW IF YOU OBSERVE AN ERROR (-40) IN RSA TEST

Begin wolfcrypt tests
MD5      test passed!
MD4      test passed!
SHA      test passed!
SHA-256  test passed!
SHA-384  test passed!
SHA-512  test passed!
HMAC-MD5 test passed!
HMAC-SHA test passed!
HMAC-SHA256 test passed!
HMAC-SHA384 test passed!
HMAC-SHA512 test passed!
GMAC     test passed!
HC-128   test passed!
Rabbit   test passed!
Chacha   test passed!
POLY1305 test passed!
ChaCha20-Poly1305 AEAD test passed!
DES      test passed!
DES3     test passed!
AES      test passed!
AES-GCM  test passed!
RANDOM   test passed!
RSA      test passed!
DH       test passed!
DSA      test passed!
PWDBASED test passed!
ECC      test passed!
wolfcrypt tests complete.

#----------------------------------------------------------------------------#
# SECTION 4:
# Evaluate benchmark tests in embOS project:
#----------------------------------------------------------------------------#

Follow the steps from section 3 only using
CUSTOM_DIR\wolfcrypt_benchmark_custom_port\

#----------------------------------------------------------------------------#
#----------------------------------------------------------------------------#

Thank you for using this guide and we hope this was helpful to you. If you have
any suggestions / feedback for us please contact us:
support@wolfssl.com
info@wolfssl.com

/* --------------------------------------------------------------------------*/
#### NOTE 1: ####

If you are working off of a base example project and you observe memory errors
when malloc is called, make sure that the linker script has set the HEAP high
enough.
Project -> Options -> Linker -> (Config Tab) -> Linker configuration file

Check this file for __size_heap__ it is typically set to 0x200 by default.
There are places in wolfSSL that malloc as much as 4k at a time and peak usage
can be as high as 29K if using full functionality.
/* --------------------------------------------------------------------------*/

Copyright © 2016 wolfSSL Inc.  All rights reserved.

