Features Configuration Bits RAM map SFR map

PIC16C765
Bank 0 | Bank 1 | Bank 3
--- | --- | ---

INDF | 0x000
TMR0 | 0x001
PCL | 0x002
STATUS | 0x003
FSR | 0x004
PORTA | 0x005
PORTB | 0x006
PORTC | 0x007
PORTD | 0x008
PORTE | 0x009
PCLATH | 0x00A
INTCON | 0x00B
PIR1 | 0x00C
PIR2 | 0x00D
TMR1TMR1L | 0x00E
TMR1H | 0x00F
T1CON | 0x010
TMR2 | 0x011
T2CON | 0x012
CCPR1CCPR1L | 0x015
CCPR1H | 0x016
CCP1CON | 0x017
RCSTA | 0x018
TXREG | 0x019
RCREG | 0x01A
CCPR2CCPR2L | 0x01B
CCPR2H | 0x01C
CCP2CON | 0x01D
ADRES | 0x01E
ADCON0 | 0x01F

OPTION_REG | 0x081
TRISA | 0x085
TRISB | 0x086
TRISC | 0x087
TRISD | 0x088
TRISE | 0x089
PIE1 | 0x08C
PIE2 | 0x08D
PCON | 0x08E
PR2 | 0x092
TXSTA | 0x098
SPBRG | 0x099
ADCON1 | 0x09F

UIR | 0x190
UIE | 0x191
UEIR | 0x192
UEIE | 0x193
USTAT | 0x194
UCTRL | 0x195
UADDR | 0x196
USWSTAT | 0x197
UEP0 | 0x198
UEP1 | 0x199
UEP2 | 0x19A
BD0OST | 0x1A0
BD0OBC | 0x1A1
BD0OAL | 0x1A2
BD0IST | 0x1A4
BD0IBC | 0x1A5
BD0IAL | 0x1A6
BD1OST | 0x1A8
BD1OBC | 0x1A9
BD1OAL | 0x1AA
BD1IST | 0x1AC
BD1IBC | 0x1AD
BD1IAL | 0x1AE
BD2OST | 0x1B0
BD2OBC | 0x1B1
BD2OAL | 0x1B2
BD2IST | 0x1B4
BD2IBC | 0x1B5
BD2IAL | 0x1B6

The mirror of [PCL, PCLATH, ...] are not shown.

SFR

SFR with alias name.

This page generated automatically by the device-help.pl program (2022-01-30 15:56:09 UTC) from the 8bit_device.info file (rev: 1.44) of mpasmx and from the gputils source package (rev: svn Unversioned directory). The mpasmx is included in the MPLAB X.