Features Configuration Bits RAM map SFR map

PIC16CE625
Coff ID of device | 0x6625
Number of ROM/FLASH pages | 1 (2048 words/pages)
Last address of ROM/FLASH | 0x07FF
Size of ROM | 2048 words
Address space of User ID | 0x2000 - 0x2003 (4 bytes)
Address of Configuration Word | 0x2007 (1 word)
Number of RAM Banks | 2 (128 bytes/banks)
Number of SFRs | 18
Size of shared GPRs | 16 bytes
Size of all GPRs | 128 bytes
Joint size of SFRs + GPRs | 146 bytes
Standard header | p16ce625.inc
Standard linker script | 16ce625_g.lkr

This page generated automatically by the device-help.pl program (2022-01-30 15:56:09 UTC) from the 8bit_device.info file (rev: 1.44) of mpasmx and from the gputils source package (rev: svn Unversioned directory). The mpasmx is included in the MPLAB X.