dnstap-read
Prev | Manual pages | Next

## Name

dnstap-read — print dnstap data in human-readable form

## Synopsis

`dnstap-read` [`-m`] [`-p`] [`-y`] {`file`}

## DESCRIPTION

dnstap-read reads dnstap data from a specified file and prints it in a human-readable format. By default, dnstap data is printed in a short summary format, but if the `-y` option is specified, then a longer and more detailed YAML format is used instead.

## OPTIONS

-m

  Trace memory allocations; used for debugging memory leaks.

-p

  After printing the dnstap data, print the text form of the DNS message that was encapsulated in the dnstap frame.

-y

  Print dnstap data in a detailed YAML format.

## SEE ALSO

named(8) , rndc(8) , BIND 9 Administrator Reference Manual.

Prev | Up | Next
arpaname | Home | genrandom

BIND 9.11.4 (Extended Support Version)